## LiteSpeed Web Server
Users' Manual

### Version 6.3 — Rev. 4

- License Enterprise
- Introduction
- Installation
- Administration
- Security
- Configuration
  - Server General
  - Server Log
  - Server Tuning
  - Server Security
  - Page Cache
  - PageSpeed Config
  - External Apps
  - Fast CGI App
  - Fast CGI Authorizer
  - LSAPI App
  - Servlet Engine
  - Web Server
  - Piped logger
  - Load Balancer
  - Script Handler
  - PHP
  - App Server Settings
  - Listener General
  - Listener SSL
  - Virtual Host Templates
  - Virtual Host Basic
  - Virtual Host General
  - Virtual Host Security
  - Virtual Host SSL
  - Virtual Host PageSpeed Config
  - Rewrite
  - Context
  - Static Context
  - Java Web App Context
  - Servlet Context
  - Fast CGI Context
  - LSAPI Context
  - Proxy Context
  - CGI Context
  - Load Balancer Context
  - Redirect Context
  - App Server Context
  - Rack/Rails Context
  - Add-ons
- Web Console
  - Admin Console General
  - Admin Console Security
  - Admin Listener General
  - Admin Listener SSL

# Admin Console Security

## Table of Contents

### Access Control⇑

#### Description

Specifies what sub networks and/or IP addresses can access the server. At the server level, this setting will affect all virtual hosts. You can also set up access control unique to each virtual host at the virtual host level. Virtual host level settings will NOT override server level settings.
Blocking/Allowing an IP is determined by the combination of the allowed list and the denied list. If you want to block only certain IPs or sub-networks, put * or ALL in the Allowed List and list the blocked IPs or sub-networks in the Denied List. If you want to allow only certain IPs or sub-networks, put * or ALL in the Denied List and list the allowed IPs or sub-networks in the Allowed List. The setting of the smallest scope that fits for an IP will be used to determine access.
Server Level: Trusted IPs or sub-networks must be specified in the Allowed List by adding a trailing "T". Trusted IPs or sub-networks are not affected by connection/throttling limits. Only server level access control can set up trusted IPs/sub-networks.

#### Tips

Use this at the server level for general restrictions that apply to all virtual hosts.

### Allowed List⇑

#### Description

Specifies the list of IPs or sub-networks allowed. * or ALL are accepted.

#### Syntax

Comma delimited list of IP addresses or sub-networks. A trailing "T" can be used to indicate a trusted IP or sub-network, such as 192.168.1.*T.

#### Example

Sub-networks: 192.168.1.0/255.255.255.0, 192.168.1.0/24, 192.168.1, or 192.168.1.*
IPv6 addresses: ::1 or [::1]
IPv6 subnets: 3ffe:302:11:2:20f:1fff:fe29:717c/64 or [3ffe:302:11:2:20f:1fff:fe29:717c]/64

#### Tips

Trusted IPs or sub-networks set at the server level access control will be excluded from connection/throttling limits.

### Denied List⇑

#### Description

Specifies the list of IPs or sub-networks disallowed.

#### Syntax

Comma delimited list of IP addresses or sub-networks. * or ALL are accepted.

#### Example

Sub-networks: 192.168.1.0/255.255.255.0, 192.168.1.0/24, 192.168.1, or 192.168.1.*
IPv6 addresses: ::1 or [::1]
IPv6 subnets: 3ffe:302:11:2:20f:1fff:fe29:717c/64 or [3ffe:302:11:2:20f:1fff:fe29:717c]/64

### WebAdmin User⇑

#### Description

Change the username and password for the WebAdmin Console. The old password must be entered and verified in order to save changes.